{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["DONNEES","DIMENSIONNEMENT","DESSIN"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"DONNEES","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,null,null,"   Radier selon B.A.E.L 91 révisé 99"]
[]
[{"$nulls":4},"NB:"," °/ N et M sont toujours positif  "]
[]
[null,null,null,"Données relative aux chargement",null,null,"Données relative au poteau"]
[]
[null,null,null,"Ns total (KN)",166968,null,"a (m)",0.45]
[null,null,null,"Nu total (KN)",227237.1,null,"b (m)",0.45]
[null,null,null,"Nu pot (KN)",3153]
[null,null,null,"Nu voile (KN)",1708.73,null,"Données relative au voile"]
[null,null,null,"Mx (KN.m)",114.52]
[null,null,null,"My (KN.m)",637.825,null,"e (m)",0.2]
[null,null,null,"N (KN)",64169.365,null,"L (m)",1]
[]
[null,null,null,"Données relative au matériau"]
[{"$nulls":6},"Caractéristique du radier"]
[null,null,null,"Fe (Mpa)"]
[null,null,null,"Fc28 (Mpa)",25,null,"Ix (m⁴)",186624]
[null,null,null,"σ'sol (Mpa)",0.2,null,"Iy (m⁴)",331776]
[{"$nulls":6},"Xg (m)",24]
[{"$nulls":6},"Yg (m)",18]
[]
[]
[null,null,null,"Hauteur de la partie ancrée du bâtiment en (m)     →",null,null,null,2]
[null,null,null,"Entre axe max entre deux élts porteurs en (m)       →",null,null,null,6]
[null,null,null,"Mauvais sol (1), Sol moyen (2), Très bon sol (3)     →",null,null,null,2]
[null,null,null,"La surface totale du bâtiment en (m²)                    →",null,null,null,1728]
[null,null,null,"Largeur du radier en (m)                                      →",null,null,null,48]
[null,null,null,"Longueur du radier en (m)                                   →",null,null,null,36]
[]
[]
[null,null,null,"Données à retenir pour le radier"]
[]
[null,null,null,"h0 (cm)",40]
[null,null,null,"h1 (cm)",150]
[null,null,null,"Srad (m²) ",1728]

{"sheet":"DIMENSIONNEMENT","index":1,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,null,null,"Dimensionnement du radier"]
[]
[null,null,null,"1°/ Pré dimensionnement du radier"]
[null,null,null,"a°/ Condition de coffrage"]
[]
[null,null,null,"h0 (cm) ≥",30]
[null,null,null,"h1 (cm) ≥",60,null,"     "]
[]
[null,null,null,45,"≤    b (cm)    ≤",105]
[]
[null,null,null,"b°/ Condition de rigidité"]
[]
[null,null,null,"E (Mpa)",32164.195]
[null,null,null,"K (KN/m³)",40000]
[null,null,null,"h1 (cm) ≥",92.607]
[]
[null,null,null,"c°/ Surface du radier"]
[]
[null,null,null,"Srad (m²) ≥",834.84]
[null,null,null,"Prendre une surface égale à celle du bâtiment"]
[null,null,null,"Ld (m) ≥",0]

{"sheet":"DESSIN","index":2,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[null,null,null,"b :","Largeur de la nervure du radier"]
[null,null,null,"h1 :","Hauteur de la nervure du radier"]
[null,null,null,"h0 :","Epaisseur de la dalle du radier"]
[null,null,null,"L1,…i :","Entre axe max entre deux élts porteurs"]
[]
[null,null,"Ns total :","Charge totale à l'ELS transmise par la superstructure plus le poids du radier"]
[null,null,"Nu total :","Charge totale à l'ELU transmise par la superstructure plus le poids du radier"]
[null,null,"Mx, My :","Moment sismique à la base du bâtiment avec la combinaison G + Q + Ex,y"]
[null,null,"N :","Poids propre du bâtiment ; uniquement la superstructure"]